<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.36.1-Maidenhead">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract></abstract>
  <links/>
  <dates/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["POSGAR 94 / Argentina 3",BASEGEOGCRS["POSGAR 94",DATUM["Posiciones Geodesicas Argentinas 1994",ELLIPSOID["WGS 84",6378137,298.257223563,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4694]],CONVERSION["Argentina zone 3",METHOD["Transverse Mercator",ID["EPSG",9807]],PARAMETER["Latitude of natural origin",-90,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8801]],PARAMETER["Longitude of natural origin",-66,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8802]],PARAMETER["Scale factor at natural origin",1,SCALEUNIT["unity",1],ID["EPSG",8805]],PARAMETER["False easting",3500000,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",0,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["northing (X)",north,ORDER[1],LENGTHUNIT["metre",1]],AXIS["easting (Y)",east,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Engineering survey, topographic mapping."],AREA["Argentina - between 67°30'W and 64°30'W, onshore."],BBOX[-55.11,-67.5,-21.78,-64.49]],ID["EPSG",22183]]</wkt>
      <proj4>+proj=tmerc +lat_0=-90 +lon_0=-66 +k=1 +x_0=3500000 +y_0=0 +ellps=WGS84 +towgs84=0,0,0,0,0,0,0 +units=m +no_defs</proj4>
      <srsid>1943</srsid>
      <srid>22183</srid>
      <authid>EPSG:22183</authid>
      <description>POSGAR 94 / Argentina 3</description>
      <projectionacronym>tmerc</projectionacronym>
      <ellipsoidacronym>EPSG:7030</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent/>
</qgis>
